edu.wpi.first.wpilibj.livewindow

## Interface LiveWindowSendable

- All Superinterfaces:
    Sendable
  All Known Subinterfaces:
    CANSpeedController
  All Known Implementing Classes:
    ADXL345_I2C, ADXL345_SPI, ADXL362, ADXRS450_Gyro, AnalogAccelerometer, AnalogGyro, AnalogInput, AnalogOutput, AnalogPotentiometer, BuiltInAccelerometer, Compressor, Counter, DigitalInput, DigitalOutput, DoubleSolenoid, Encoder, GearTooth, GyroBase, Jaguar, PIDController, PowerDistributionPanel, PWM, PWMSpeedController, PWMTalonSRX, Relay, SafePWM, SD540, Servo, Solenoid, Spark, Talon, Ultrasonic, Victor, VictorSP

      public interface LiveWindowSendable
      extends Sendable

  Live Window Sendable is a special type of object sendable to the live window.

- - ### Method Summary

    All Methods Instance Methods Abstract Methods
    Modifier and Type | Method and Description
    --- | ---
    `void` | `startLiveWindowMode()` Start having this sendable object automatically respond to value changes reflect the value on the table.
    `void` | `stopLiveWindowMode()` Stop having this sendable object automatically respond to value changes.
    `void` | `updateTable()` Update the table for this sendable object with the latest values.

    - ### Methods inherited from interface edu.wpi.first.wpilibj.Sendable

      `getSmartDashboardType, initTable`

- - ### Method Detail

    - #### updateTable

          void updateTable()

      Update the table for this sendable object with the latest values.

    - #### startLiveWindowMode

          void startLiveWindowMode()

      Start having this sendable object automatically respond to value changes reflect the value on the table.

    - #### stopLiveWindowMode

          void stopLiveWindowMode()

      Stop having this sendable object automatically respond to value changes.