REM This is BadKB demo script for windows

REM Open windows notepad
DELAY 1000
GUI r
DELAY 500
STRING notepad
DELAY 500
ENTER
DELAY 750

STRING Hello World!
ENTER
DEFAULT_DELAY 50

REM Copy-Paste previous string
UP
HOME
SHIFT DOWN
CTRL c
RIGHT
CTRL v
CTRL v

REM Alt code input demo
ALTCHAR 7
ALTSTRING This line was print using Alt+Numpad input method. It works even if non-US keyboard layout is selected
ENTER

STRING =
REPEAT 59
ENTER
ENTER

STRING               _.-------.._                    -,
ENTER
HOME
STRING           .-"```"--..,,_/ /`-,               -,  \ 
ENTER
HOME
STRING        .:"          /:/  /'\  \     ,_...,  `. |  |
ENTER
HOME
STRING       /       ,----/:/  /`\ _\~`_-"`     _;
ENTER
HOME
STRING      '      / /`"""'\ \ \.~`_-'      ,-"'/ 
ENTER
HOME
STRING     |      | |  0    | | .-'      ,/`  /
ENTER
HOME
STRING    |    ,..\ \     ,.-"`       ,/`    /
ENTER
HOME
STRING   ;    :    `/`""\`           ,/--==,/-----,
ENTER
HOME
STRING   |    `-...|        -.___-Z:_______J...---;
ENTER
HOME
STRING   :         `                           _-'
ENTER
HOME
STRING  _L_  _     ___  ___  ___  ___  ____--"`
ENTER
HOME
STRING | __|| |   |_ _|| _ \| _ \| __|| _ \ 
ENTER
HOME
STRING | _| | |__  | | |  _/|  _/| _| |   / 
ENTER
HOME
STRING |_|  |____||___||_|  |_|  |___||_|_\ 
ENTER
HOME
ENTER

STRING Flipper Zero BadKB feature is compatible with USB Rubber Ducky script format
ENTER
STRING More information about script syntax can be found here:
ENTER
STRING https://github.com/flipperdevices/flipperzero-firmware/blob/dev/documentation/file_formats/BadUsbScriptFormat.md
ENTER
