Retro Rocket Kernel BASIC-Powered Operating System

Data Fields
ahci_fis_reg_h2d_t Struct Reference

`#include <ahci.h>`

Collaboration diagram for ahci_fis_reg_h2d_t:
[legend]

## Data Fields
uint8_t | fis_type
uint8_t | pmport:4
uint8_t | rsv0:3
uint8_t | c:1
uint8_t | command
uint8_t | featurel
uint8_t | lba0
uint8_t | lba1
uint8_t | lba2
uint8_t | device
uint8_t | lba3
uint8_t | lba4
uint8_t | lba5
uint8_t | featureh
uint8_t | countl
uint8_t | counth
uint8_t | icc
uint8_t | control
uint8_t | rsv1 [4]

## Field Documentation

## ◆ c

uint8_t ahci_fis_reg_h2d_t::c

## ◆ command

uint8_t ahci_fis_reg_h2d_t::command

## ◆ control

uint8_t ahci_fis_reg_h2d_t::control

## ◆ counth

uint8_t ahci_fis_reg_h2d_t::counth

## ◆ countl

uint8_t ahci_fis_reg_h2d_t::countl

## ◆ device

uint8_t ahci_fis_reg_h2d_t::device

## ◆ featureh

uint8_t ahci_fis_reg_h2d_t::featureh

## ◆ featurel

uint8_t ahci_fis_reg_h2d_t::featurel

## ◆ fis_type

uint8_t ahci_fis_reg_h2d_t::fis_type

## ◆ icc

uint8_t ahci_fis_reg_h2d_t::icc

## ◆ lba0

uint8_t ahci_fis_reg_h2d_t::lba0

## ◆ lba1

uint8_t ahci_fis_reg_h2d_t::lba1

## ◆ lba2

uint8_t ahci_fis_reg_h2d_t::lba2

## ◆ lba3

uint8_t ahci_fis_reg_h2d_t::lba3

## ◆ lba4

uint8_t ahci_fis_reg_h2d_t::lba4

## ◆ lba5

uint8_t ahci_fis_reg_h2d_t::lba5

## ◆ pmport

uint8_t ahci_fis_reg_h2d_t::pmport

## ◆ rsv0

uint8_t ahci_fis_reg_h2d_t::rsv0

## ◆ rsv1

uint8_t ahci_fis_reg_h2d_t::rsv1[4]