Retro Rocket Kernel BASIC-Powered Operating System

Data Fields
ahci_fis_reg_d2h_t Struct Reference

`#include <ahci.h>`

Collaboration diagram for ahci_fis_reg_d2h_t:
[legend]

## Data Fields
uint8_t | fis_type
uint8_t | pmport:4
uint8_t | rsv0:2
uint8_t | i:1
uint8_t | rsv1:1
uint8_t | status
uint8_t | error
uint8_t | lba0
uint8_t | lba1
uint8_t | lba2
uint8_t | device
uint8_t | lba3
uint8_t | lba4
uint8_t | lba5
uint8_t | rsv2
uint8_t | countl
uint8_t | counth
uint8_t | rsv3 [2]
uint8_t | rsv4 [4]

## Field Documentation

## ◆ counth

uint8_t ahci_fis_reg_d2h_t::counth

## ◆ countl

uint8_t ahci_fis_reg_d2h_t::countl

## ◆ device

uint8_t ahci_fis_reg_d2h_t::device

## ◆ error

uint8_t ahci_fis_reg_d2h_t::error

## ◆ fis_type

uint8_t ahci_fis_reg_d2h_t::fis_type

## ◆ i

uint8_t ahci_fis_reg_d2h_t::i

## ◆ lba0

uint8_t ahci_fis_reg_d2h_t::lba0

## ◆ lba1

uint8_t ahci_fis_reg_d2h_t::lba1

## ◆ lba2

uint8_t ahci_fis_reg_d2h_t::lba2

## ◆ lba3

uint8_t ahci_fis_reg_d2h_t::lba3

## ◆ lba4

uint8_t ahci_fis_reg_d2h_t::lba4

## ◆ lba5

uint8_t ahci_fis_reg_d2h_t::lba5

## ◆ pmport

uint8_t ahci_fis_reg_d2h_t::pmport

## ◆ rsv0

uint8_t ahci_fis_reg_d2h_t::rsv0

## ◆ rsv1

uint8_t ahci_fis_reg_d2h_t::rsv1

## ◆ rsv2

uint8_t ahci_fis_reg_d2h_t::rsv2

## ◆ rsv3

uint8_t ahci_fis_reg_d2h_t::rsv3[2]

## ◆ rsv4

uint8_t ahci_fis_reg_d2h_t::rsv4[4]

## ◆ status

uint8_t ahci_fis_reg_d2h_t::status