    // Set ASPM of PCI0.RP05(WiFi) to L1
    DefinitionBlock ("", "SSDT", 2, "OCLT", "ASPM", 0)
    {
        External (_SB.PCI0.RP05, DeviceObj)
        Scope (_SB.PCI0.RP05)
        {
            OperationRegion (LLLL, PCI_Config, 0x50, 1)
            Field (LLLL, AnyAcc, NoLock, Preserve)
            {
                L1,   1
            }
        }

        Scope (\)
        {
            If (_OSI ("Darwin"))
            {
                \_SB.PCI0.RP05.L1 = Zero   //Set ASPM = L1
            }
        }
    }
    //EOF

# results matching ""

# No results matching ""