# SmartcardSAM Module

class `virtualsmartcard.SmartcardSAM.``SAM`(PIN, cardNumber, mf=None, cardSecret=None, default_se=<class 'virtualsmartcard.SEutils.Security_Environment'>)

  Bases: `object`

  This class is used to store the data needed by the SAM. It includes the PIN, the master key of the SAM and a hashmap containing all the keys used by the file encryption system. The keys in the hashmap are indexed via the path to the corresponding container.

  `FSdecrypt`(data)

    Decrypt the given data, using the parameters stored in the SAM. Right now we do not encrypt the data. In memory encryption might or might not be added in a future version.

  `FSencrypt`(data)

    Encrypt the given data, using the parameters stored in the SAM. Right now we do not encrypt the data. In memory encryption might or might not be added in a future version.

  `_get_referenced_key`(p1, p2)

    This method returns the key specified by the p2 parameter. The key may be stored on the cards filesystem.

    Parameters

      - p1 – Specifies the algorithm to use.

      - p2 –

        Specifies a reference to the key to be used for encryption.

        b8 | b7 | b6 | b5 | b4 | b3 | b2 | b1 | Meaning
        --- | --- | --- | --- | --- | --- | --- | --- | ---
        0 | 0 | 0 | 0 | 0 | 0 | 0 | 0 | No information is given
        0 |  |  |  |  |  |  |  | Global reference data(e.g. MF specific key)
        1 |  |  |  |  |  |  |  | Specific reference data(e.g. DF specific key)
        |  |  | x | x | x | x | x | Number of the secret

        Any other value RFU

  `change_reference_data`(p1, p2, data)

    Change the specified referenced data (e.g. CHV) of the card

  `erase_SE`(SEID)

    Erases a Security Environment stored under SEID from the SAM

  `external_authenticate`(p1, p2, data)

    Authenticate the terminal to the card. Check whether Terminal correctly encrypted the given challenge or not

  `generate_public_key_pair`(p1, p2, data)
  `get_card_number`()
  `get_challenge`(p1, p2, data)

    Generate a random number of maximum 8 Byte and return it.

  `internal_authenticate`(p1, p2, data)

    Authenticate card to terminal. Encrypt the challenge of the terminal to prove key posession

  `manage_security_environment`(p1, p2, data)
  `mutual_authenticate`(p1, p2, mutual_challenge)

    Takes an encrypted challenge in the form ‘Terminal Challenge | Card Challenge | Card number’ and checks it for validity. If the challenge is successful the card encrypts ‘Card Challenge | Terminal challenge’ and returns this value

  `parse_SM_CAPDU`(CAPDU, header_authentication)

    Parse a command APDU protected by Secure Messaging and return the unprotected command APDU

  `perform_security_operation`(p1, p2, data)
  `protect_result`(sw, unprotected_result)

    Protect a plain response APDU by Secure Messaging

  `restore_SE`(SEID)

    Restores a Security Environment from the SAM and replaces the current SE with it.

  `set_MF`(mf)

    Setter function for the internal reference to the Filesystem. The SAM needs a reference to the filesystem in order to store/retrieve keys.

  `set_asym_algorithm`(cipher, keytype)
    Parameters

      - cipher – Public/private key object from used for encryption

      - keytype – Type of the public key (e.g. RSA, DSA)

  `store_SE`(SEID)

    Stores the current Security environment in the secure access module. The SEID is used as a reference to identify the SE.

  `verify`(p1, p2, PIN)

    Authenticate the card user. Check if he entered a valid PIN. If the PIN is invalid decrement retry counter. If retry counter equals zero, block the card until reset with correct PUK

`virtualsmartcard.SmartcardSAM.``get_referenced_cipher`(p1)

  P1 defines the algorithm and mode to use. We dispatch it and return a string that is understood by CryptoUtils.py functions