Type | Name | Quantity | Case | Comment
R | 10k ¼W | 2 |  |
R | 1k ¼W | 20 |  |
R | 100 ¼W | 1 |  |
R | 22R ¼W | 1 |  |
R | 10R ¼W | 1 |  |
Cap | 0.1 uf | 4 |  |
Cap | 22uf_16v | 4 |  |
IC | PC817C | 1 or 4 | DIP-4 | 1pcs if you use inputs as buttons, else: 4pcs
Conn | DIP-16 bed | 2 | DIP-16 |
IC | ULN2003APG | 2 | DIP-16 |
IC | 7805 TO-220 | 1 | TO-220 |
IC | 2n2222 | 1 | TO-92 |
- | SMIH-12VDC-SL-C | 2 |  |
- | SRD-12VDC-SL-C | 3 |  |
Module | TTL_485_MODULE_8PIN | 1 |  |
Module | ARDUINO PRO MINI 328P 5V | 1 |  |
Conn | KF128 2.54_screw_3P | 1 |  |
Conn | KF128 2.54_screw_12P | 2 |  |
Conn | KF128 3.81_screw_2P | 7 |  |
Conn | KF128 5.08_screw_2P | 3 |  |
Conn | 2.54_legs_female_2P | 1 |  |
Conn | 2.54_legs_female_3P | 1 |  |
Conn | 2.54_legs_female_4P | 2 |  |
Conn | 2.54_legs_female_12P | 2 |  |
Conn | 2.54_male_pins_40 | 1 |  | array of male pins to cut to custom sizes
LED | LED-2*5*7 | 5 |  |
Button | momentary switch 6x6x2 | 3 |  | 3pcs if you use buttons
Display | 1602 LCD with i2c interface | 1 |  | optional
- | buzzer | 1 | R9.0-2P-4.0PITCH |
Module | LM2596S module | 0 or 1 | XX-to-12 stab | Needed only if you will use 24v as power source
- | power source, 12v1.25A 70x30x40 | 1 | 70x30x40 |
- | ds18b20 | 6 |  | 1 to 13, 6 recommended as fast start
| usb→uart | 1 |  | To upload firmware
- | current sensor sct-013-000 | 1 |  |
| rs485-USB | 1 |  | To connect CHPC < - > PC/notebook