----------------------------
title : VEXPANDPD (Intel x86/64 assembly instruction)
cat_title : VEXPANDPD
ref_title : VEXPANDPD
published : 2020-09-01
path : /X86-64 명령어 레퍼런스/V
publish_date: 2020-09-01
----------------------------


#@ VEXPANDPD

**Load Sparse Packed Double-Precision Floating-Point Values from Dense Memory**

```lec-info
아래 표를 해석하는 방법은 [x86-64 명령어 레퍼런스 읽는 법](/316) 글을 참조하시기 바랍니다.
```

|**Opcode/**\newline{}**Instruction**|**Op / **\newline{}**En**|**64/32 **\newline{}**bit Mode **\newline{}**Support**|**CPUID **\newline{}**Feature **\newline{}**Flag**|**Description**|
|------------------------------------|-------------------------|------------------------------------------------------|--------------------------------------------------|---------------|
|`EVEX.128.66.0F38.W1 88 /r`\newline{}`VEXPANDPD` \tooltip{xmm1}{128 비트 XMM 레지스터로 XMM0 부터 XMM7 까지 있다. 64 비트 모드에서는 XMM8 부터 XMM15 까지 추가적으로 사용할 수 있다.} \tooltip{\{k1\}\{z\}}{쓰기 마스크 (write mask) 레지스터로 64 비트 k 레지스터로 k1 부터 k7 까지 사용 가능하다. 쓰기 마스크는 오직 EVEX 접두사가 있을 경우에만 사용 가능하다. 마스크 방식으로 마스크 되지 않는 부분의 값을 유지하는 병합 마스크 (merge mask) 가 있고, 해당 부분을 아예 0 으로 지워버리는 zeroing mask 방식이 있다. 어떤 식으로 마스크를 할 지는 EVEX.z 필드의 비트값에 따라 달라진다.} \tooltip{xmm2/m128}{128 비트 XMM 레지스터 혹은 128 비트 메모리 데이터.} |T1S|V/V|AVX512VL\newline{}AVX512F|Expand packed double-precision floating-point values from xmm2/m128 to xmm1 using writemask k1.|
|`EVEX.256.66.0F38.W1 88 /r`\newline{}`VEXPANDPD` \tooltip{ymm1}{256 비트 YMM 레지스터로 YMM0 부터 YMM7 까지 있다. 64 비트 모드에서는 YMM8 부터 YMM15 까지 추가적으로 사용할 수 있다.} \tooltip{\{k1\}\{z\}}{쓰기 마스크 (write mask) 레지스터로 64 비트 k 레지스터로 k1 부터 k7 까지 사용 가능하다. 쓰기 마스크는 오직 EVEX 접두사가 있을 경우에만 사용 가능하다. 마스크 방식으로 마스크 되지 않는 부분의 값을 유지하는 병합 마스크 (merge mask) 가 있고, 해당 부분을 아예 0 으로 지워버리는 zeroing mask 방식이 있다. 어떤 식으로 마스크를 할 지는 EVEX.z 필드의 비트값에 따라 달라진다.} \tooltip{ymm2/m256}{YMM 레지스터나 256 비트 메모리 데이터.} |T1S|V/V|AVX512VL\newline{}AVX512F|Expand packed double-precision floating-point values from ymm2/m256 to ymm1 using writemask k1.|
|`EVEX.512.66.0F38.W1 88 /r`\newline{}`VEXPANDPD` zmm1 \tooltip{\{k1\}\{z\}}{쓰기 마스크 (write mask) 레지스터로 64 비트 k 레지스터로 k1 부터 k7 까지 사용 가능하다. 쓰기 마스크는 오직 EVEX 접두사가 있을 경우에만 사용 가능하다. 마스크 방식으로 마스크 되지 않는 부분의 값을 유지하는 병합 마스크 (merge mask) 가 있고, 해당 부분을 아예 0 으로 지워버리는 zeroing mask 방식이 있다. 어떤 식으로 마스크를 할 지는 EVEX.z 필드의 비트값에 따라 달라진다.} \tooltip{zmm2/m512}{ZMM 레지스터나 512 비트 메모리 데이터.} |T1S|V/V|AVX512F|Expand packed double-precision floating-point values from zmm2/m512 to zmm1 using writemask k1.|
### Instruction Operand Encoding


|Op/En|Operand 1|Operand 2|Operand 3|Operand 4|
|-----|---------|---------|---------|---------|
|T1S|ModRM:reg (w)|ModRM:r/m (r)|NA|NA|
### Description 


Expand (load) up to 8/4/2, contiguous, double-precision floating-point values of the input vector in the source operand (the second operand) to sparse elements in the destination operand (the first operand) selected by the writemask k1. 

The destination operand is a ZMM/YMM/XMM register, the source operand can be a ZMM/YMM/XMM register or a 512/256/128-bit memory location.

The input vector starts from the lowest element in the source operand. The writemask register k1 selects the desti-nation elements (a partial vector or sparse elements if less than 8 elements) to be replaced by the ascending elements in the input vector. Destination elements not selected by the writemask k1 are either unmodified or zeroed, depending on EVEX.z.

EVEX.vvvv is reserved and must be 1111b otherwise instructions will #UD.

Note that the compressed displacement assumes a pre-scaling (N) corresponding to the size of one single element instead of the size of the full vector.


### Operation
#### VEXPANDPD (EVEX encoded versions) 
```info-verb
(KL, VL) = (2, 128), (4, 256), (8, 512)
k <-  0
FOR j <-  0 TO KL-1
    i <-  j * 64
    IF k1[j] OR *no writemask*
          THEN 
                DEST[i+63:i] <-  SRC[k+63:k];
                k <-  k + 64
          ELSE 
                IF *merging-masking* ; merging-masking
                      THEN *DEST[i+63:i] remains unchanged*
                      ELSE  ; zeroing-masking
                            THEN DEST[i+63:i] <-  0
                FI
    FI;
ENDFOR
DEST[MAX_VL-1:VL] <-!= 0
```

### Intel C/C++ Compiler Intrinsic Equivalent

```cpp
VEXPANDPD __m512d _mm512_mask_expand_pd( __m512d s, __mmask8 k, __m512d a);
VEXPANDPD __m512d _mm512_maskz_expand_pd( __mmask8 k, __m512d a);
VEXPANDPD __m512d _mm512_mask_expandloadu_pd( __m512d s, __mmask8 k, void * a);
VEXPANDPD __m512d _mm512_maskz_expandloadu_pd( __mmask8 k, void * a);
VEXPANDPD __m256d _mm256_mask_expand_pd( __m256d s, __mmask8 k, __m256d a);
VEXPANDPD __m256d _mm256_maskz_expand_pd( __mmask8 k, __m256d a);
VEXPANDPD __m256d _mm256_mask_expandloadu_pd( __m256d s, __mmask8 k, void * a);
VEXPANDPD __m256d _mm256_maskz_expandloadu_pd( __mmask8 k, void * a);
VEXPANDPD __m128d _mm_mask_expand_pd( __m128d s, __mmask8 k, __m128d a);
VEXPANDPD __m128d _mm_maskz_expand_pd( __mmask8 k, __m128d a);
VEXPANDPD __m128d _mm_mask_expandloadu_pd( __m128d s, __mmask8 k, void * a);
VEXPANDPD __m128d _mm_maskz_expandloadu_pd( __mmask8 k, void * a);
```
### SIMD Floating-Point Exceptions


None

### Other Exceptions


See Exceptions Type E4.nb.

#UD If EVEX.vvvv != 1111B.

