----------------------------
title : BTC (Intel x86/64 assembly instruction)
cat_title : BTC
ref_title : BTC
published : 2020-09-01
path : /X86-64 명령어 레퍼런스/B
publish_date: 2020-09-01
----------------------------


#@ BTC

**Bit Test and Complement**

```lec-info
아래 표를 해석하는 방법은 [x86-64 명령어 레퍼런스 읽는 법](/316) 글을 참조하시기 바랍니다.
```

|**Opcode**|**Instruction**|**Op/ **\newline{}**En**|**64-bit **\newline{}**Mode**|**Compat/**\newline{}**Leg Mode**|**Description**|
|----------|---------------|------------------------|-----------------------------|---------------------------------|---------------|
|0F BB /r|`BTC` \tooltip{r/m16}{2 바이트 짜리 피연산자로, 2 바이트 범용 레지스터나 (r16 의 레지스터들), 2 바이트 메모리 데이터를 의미한다. } \tooltip{r16}{2 바이트 짜리 범용 레지스터를 의미 (AX, CX, DX, BX, SP, BP, SI, DI). 64 비트 모드의 경우 추가적으로 R8 부터 R15 까지 가능.} |MR|Valid|Valid|Store selected bit in CF flag and complement.|
|0F BB /r|`BTC` \tooltip{r/m32}{4 바이트 짜리 피연산자로, 4 바이트 범용 레지스터나 (r32 의 레지스터들), 4 바이트 메모리 데이터를 의미한다.} \tooltip{r32}{4 바이트 짜리 범용 레지스터를 의미 (EAX, ECX, EDX, EBX, ESP, EBP, ESI, EDI). 64 비트 모드의 경우 추가적으로 R8D 부터 R15D 까지 가능.} |MR|Valid|Valid|Store selected bit in CF flag and complement.|
|REX.W + 0F BB /r|`BTC` \tooltip{r/m64}{8 바이트 짜리 피연산자로, 8 바이트 범용 레지스터나 (r64 의 레지스터들), 8 바이트 메모리 데이터를 의미한다.} \tooltip{r64}{8 바이트 짜리 범용 레지스터를 의미 (RAX, RBX, RCX, RDX, RDI, RSI, RBP, RSP, R8–R15). 이들은 64비트 모드에서만 사용 가능하다.} |MR|Valid|N.E.|Store selected bit in CF flag and complement.|
|0F BA /7 ib|`BTC` \tooltip{r/m16}{2 바이트 짜리 피연산자로, 2 바이트 범용 레지스터나 (r16 의 레지스터들), 2 바이트 메모리 데이터를 의미한다. } \tooltip{imm8}{1 바이트 짜리 명시적 데이터 (immediate value). imm8 의 경우 부호 있는 정수를 의미하며, -128 부터 127 까지의 값을 표현할 수 있다. 참고로 만일 imm8 이 1 바이트 보다 큰 피연산자를 가지는 명령어와 사용될 경우, 명시적 데이터는 부호를 유지한채 해당 크기로 확장이 된다. (쉽게 말해 0b11000000 은 0b11111111 11000000 로 확장되며 0b00110000 은 0b00000000 00110000 으로 확장된다.)} |MI|Valid|Valid|Store selected bit in CF flag and complement.|
|0F BA /7 ib|`BTC` \tooltip{r/m32}{4 바이트 짜리 피연산자로, 4 바이트 범용 레지스터나 (r32 의 레지스터들), 4 바이트 메모리 데이터를 의미한다.} \tooltip{imm8}{1 바이트 짜리 명시적 데이터 (immediate value). imm8 의 경우 부호 있는 정수를 의미하며, -128 부터 127 까지의 값을 표현할 수 있다. 참고로 만일 imm8 이 1 바이트 보다 큰 피연산자를 가지는 명령어와 사용될 경우, 명시적 데이터는 부호를 유지한채 해당 크기로 확장이 된다. (쉽게 말해 0b11000000 은 0b11111111 11000000 로 확장되며 0b00110000 은 0b00000000 00110000 으로 확장된다.)} |MI|Valid|Valid|Store selected bit in CF flag and complement.|
|REX.W + 0F BA /7 ib|`BTC` \tooltip{r/m64}{8 바이트 짜리 피연산자로, 8 바이트 범용 레지스터나 (r64 의 레지스터들), 8 바이트 메모리 데이터를 의미한다.} \tooltip{imm8}{1 바이트 짜리 명시적 데이터 (immediate value). imm8 의 경우 부호 있는 정수를 의미하며, -128 부터 127 까지의 값을 표현할 수 있다. 참고로 만일 imm8 이 1 바이트 보다 큰 피연산자를 가지는 명령어와 사용될 경우, 명시적 데이터는 부호를 유지한채 해당 크기로 확장이 된다. (쉽게 말해 0b11000000 은 0b11111111 11000000 로 확장되며 0b00110000 은 0b00000000 00110000 으로 확장된다.)} |MI|Valid|N.E.|Store selected bit in CF flag and complement.|
### Instruction Operand Encoding


|Op/En|Operand 1|Operand 2|Operand 3|Operand 4|
|-----|---------|---------|---------|---------|
|MR|ModRM:r/m (r, w)|ModRM:reg (r)|NA|NA|
|MI|ModRM:r/m (r, w)|imm8|NA|NA|
### Description


Selects the bit in a bit string (specified with the first operand, called the bit base) at the bit-position designated by the bit offset operand (second operand), stores the value of the bit in the CF flag, and complements the selected bit in the bit string. The bit base operand can be a register or a memory location; the bit offset operand can be a register or an immediate value:

*  If the bit base operand specifies a register, the instruction takes the modulo 16, 32, or 64 of the bit offset operand (modulo size depends on the mode and register size; 64-bit operands are available only in 64-bit mode). This allows any bit position to be selected. 

*  If the bit base operand specifies a memory location, the operand represents the address of the byte in memory that contains the bit base (bit 0 of the specified byte) of the bit string. The range of the bit position that can be referenced by the offset operand depends on the operand size.

See also: Bit(BitBase, BitOffset) on page 3-11. 

Some assemblers support immediate bit offsets larger than 31 by using the immediate bit offset field in combina-tion with the displacement field of the memory operand. See "BT--Bit Test" in this chapter for more information on this addressing mechanism.

This instruction can be used with a `LOCK` prefix to allow the instruction to be executed atomically.

In 64-bit mode, the instruction's default operation size is 32 bits. Using a REX prefix in the form of REX.R permits access to additional registers (R8-R15). Using a REX prefix in the form of REX.W promotes operation to 64 bits. See the summary chart at the beginning of this section for encoding data and limits.


### Operation

```info-verb
CF <- Bit(BitBase, BitOffset);
Bit(BitBase, BitOffset) <- NOT Bit(BitBase, BitOffset);
```
### Flags Affected


The CF flag contains the value of the selected bit before it is complemented. The ZF flag is unaffected. The OF, SF, AF, and PF flags are undefined.


### Protected Mode Exceptions

#### #GP(0)
* If the destination operand points to a non-writable segment.
* If a memory operand effective address is outside the CS, DS, ES, FS, or GS segment limit.
* If the DS, ES, FS, or GS register contains a NULL segment selector.

#### #SS(0)
* If a memory operand effective address is outside the SS segment limit.

#### #PF(fault-code)
* If a page fault occurs.

#### #AC(0)
* If alignment checking is enabled and an unaligned memory reference is made while the current privilege level is 3.

#### #UD
* If the LOCK prefix is used but the destination is not a memory operand.

### Real-Address Mode Exceptions

#### #GP
* If a memory operand effective address is outside the CS, DS, ES, FS, or GS segment limit.

#### #SS
* If a memory operand effective address is outside the SS segment limit.

#### #UD
* If the LOCK prefix is used but the destination is not a memory operand.

### Virtual-8086 Mode Exceptions

#### #GP(0)
* If a memory operand effective address is outside the CS, DS, ES, FS, or GS segment limit.

#### #SS(0)
* If a memory operand effective address is outside the SS segment limit.

#### #PF(fault-code)
* If a page fault occurs.

#### #AC(0)
* If alignment checking is enabled and an unaligned memory reference is made.

#### #UD
* If the LOCK prefix is used but the destination is not a memory operand.

### Compatibility Mode Exceptions



Same exceptions as in protected mode.


### 64-Bit Mode Exceptions

#### #SS(0)
* If a memory address referencing the SS segment is in a non-canonical form.

#### #GP(0)
* If the memory address is in a non-canonical form.

#### #PF(fault-code)
* If a page fault occurs.

#### #AC(0)
* If alignment checking is enabled and an unaligned memory reference is made while the current privilege level is 3.

#### #UD
* If the LOCK prefix is used but the destination is not a memory operand.
