
Booting...


@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@

@

@ chip__no chip__id mfr___id dev___id cap___id size_sft dev_size chipSize

@ 0000000h 0ef4016h 00000efh 0000040h 0000016h 0000000h 0000016h 0400000h

@ blk_size blk__cnt sec_size sec__cnt pageSize page_cnt chip_clk chipName

@ 0010000h 0000040h 0001000h 0000400h 0000100h 0000010h 000002dh W25Q32

@ 

@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@@

DDR2:64MB

 

---RealTek(RTL8196D)at 2019.02.21-13:17+0800 v1.4a [16bit](659MHz)

no sys signature at 00010000!

no sys signature at 00020000!

no sys signature at 00030000!

no sys signature at 00017000!

no rootfs signature at 000E0000!

no rootfs signature at 000F0000!

no rootfs signature at 00130000!

no rootfs signature at 00137000!

Jump to image start=0x80500000...

decompressing kernel:
Uncompressing Linux... done, booting the kernel.
done decompressing kernel.
start address: 0x80003400
Realtek WLAN driver - version 1.7 (2015-10-30)(SVN:1846)
DFS function - version 2.0.6
Adaptivity function - version 9.3.2


#######################################################
SKB_BUF_SIZE=3600 MAX_SKB_NUM=768
#######################################################



#######################################################
SKB_BUF_SIZE=3600 MAX_SKB_NUM=768
#######################################################




Probing RTL8186 10/100 NIC-kenel stack size order[3]...
chip name: 8196C, chip revid: 0
NOT YET
eth0 added. vid=9 Member port 0x1...
eth1 added. vid=8 Member port 0x10...
eth2 added. vid=9 Member port 0x2...
eth3 added. vid=9 Member port 0x4...
eth4 added. vid=9 Member port 0x8...
eth5 added. vid=9 Member port 0x0...
[peth0] added, mapping to [eth1]...
Realtek FastPath:v1.03

init started: BusyBox v1.13.4 (2019-02-21 13:17:44 CST)
errno:13
Init Start...
Init bridge interface...


************* Initialize MAC/PHY parameter *************
[MAC_REG_8812_n]
[PHY_REG_8812_n_hp]
[PHY_REG_PG_8812]
[AGC_TAB_8812_n_hp]
[RadioA_8812_n_hp]
[RadioB_8812_n_hp]
[REG_TXPWR_TRK_8812_hp]


************* Initialize MAC/PHY parameter *************
Init Wlan application...

WiFi Simple Config v2.18-wps2.0 (2015.11.09-07:03+0000).

Register to wlan0
Register to wlan1
route: SIOCDELRT: No such process
open fifo /var/iapp.fifo OK
open fifo /var/wscd-wlan0.fifo OK
open fifo /var/wscd-wlan1.fifo OK
iwcontrol RegisterPID to (wlan0)
iwcontrol RegisterPID to (wlan1)
IEEE 802.11f (IAPP) using interface br0 (v1.8)
Init WAN Interface...
Start setting IPv6[IPv6]
boa: server version Boa

WRT-1200AC login: 