| LibDriver MPU9250 1.0.0 MPU9250 full function driver

Data Fields
mpu9250_info_s Struct Reference
mpu9250 driver function » mpu9250 basic driver function

mpu9250 information structure definition More...

`#include <driver_mpu9250.h>`

## Data Fields
char | chip_name [32]
char | manufacturer_name [32]
char | interface [8]
float | supply_voltage_min_v
float | supply_voltage_max_v
float | max_current_ma
float | temperature_min
float | temperature_max
uint32_t | driver_version

## Detailed Description

mpu9250 information structure definition

Definition at line 530 of file driver_mpu9250.h.

## Field Documentation

## ◆ chip_name

char chip_name[32]

chip name

Definition at line 532 of file driver_mpu9250.h.

## ◆ driver_version

uint32_t driver_version

driver version

Definition at line 540 of file driver_mpu9250.h.

## ◆ interface

char interface[8]

chip interface name

Definition at line 534 of file driver_mpu9250.h.

## ◆ manufacturer_name

char manufacturer_name[32]

manufacturer name

Definition at line 533 of file driver_mpu9250.h.

## ◆ max_current_ma

float max_current_ma

chip max current

Definition at line 537 of file driver_mpu9250.h.

## ◆ supply_voltage_max_v

float supply_voltage_max_v

chip max supply voltage

Definition at line 536 of file driver_mpu9250.h.

## ◆ supply_voltage_min_v

float supply_voltage_min_v

chip min supply voltage

Definition at line 535 of file driver_mpu9250.h.

## ◆ temperature_max

float temperature_max

chip max operating temperature

Definition at line 539 of file driver_mpu9250.h.

## ◆ temperature_min

float temperature_min

chip min operating temperature

Definition at line 538 of file driver_mpu9250.h.

The documentation for this struct was generated from the following file:

- src/driver_mpu9250.h