| LibDriver MPU9250 1.0.0 MPU9250 full function driver

driver_mpu9250_dmp_tap_orient_motion_test.h
Go to the documentation of this file.
1
37 #ifndef DRIVER_MPU9250_DMP_TAP_ORIENT_MOTION_TEST_H
38 #define DRIVER_MPU9250_DMP_TAP_ORIENT_MOTION_TEST_H
39
40 #include "driver_mpu9250_interface.h"
41
42 #ifdef __cplusplus
43 extern "C"{
44 #endif
45
58 uint8_t mpu9250_dmp_tap_orient_motion_test_irq_handler(void);
59
69 uint8_t mpu9250_dmp_tap_orient_motion_test(mpu9250_interface_t interface, mpu9250_address_t addr);
70
75 #ifdef __cplusplus
76 }
77 #endif
78
79 #endif
driver_mpu9250_interface.h
driver mpu9250 interface header file
mpu9250_address_t
mpu9250_address_t
mpu9250 address enumeration definition
Definition: driver_mpu9250.h:72
mpu9250_interface_t
mpu9250_interface_t
mpu9250 interface enumeration definition
Definition: driver_mpu9250.h:63
mpu9250_dmp_tap_orient_motion_test_irq_handler
uint8_t mpu9250_dmp_tap_orient_motion_test_irq_handler(void)
dmp tap orient motion test irq
Definition: driver_mpu9250_dmp_tap_orient_motion_test.c:58
mpu9250_dmp_tap_orient_motion_test
uint8_t mpu9250_dmp_tap_orient_motion_test(mpu9250_interface_t interface, mpu9250_address_t addr)
dmp test
Definition: driver_mpu9250_dmp_tap_orient_motion_test.c:231