Verify that the kernel is not crashed with receiving and sending UDP datagram
at the different NICs with the following conditions

udp4-multi-diffnic01
	IPv4

udp4-multi-diffnic02
	IPv4
	IPsec [ AH / transport ]

udp4-multi-diffnic03
	IPv4
	IPsec [ AH / tunnel ]

udp4-multi-diffnic04
	IPv4
	IPsec [ ESP / transport ]

udp4-multi-diffnic05
	IPv4
	IPsec [ ESP / tunnel ]

udp4-multi-diffnic06
	IPv4
	IPcomp [ transport ]

udp4-multi-diffnic07
	IPv4
	IPcomp [ tunnel ]

udp6-multi-diffnic01
	IPv6

udp6-multi-diffnic02
	IPv6
	IPsec [ AH / transport ]

udp6-multi-diffnic03
	IPv6
	IPsec [ AH / tunnel ]

udp6-multi-diffnic04
	IPv6
	IPsec [ ESP / transport ]

udp6-multi-diffnic05
	IPv6
	IPsec [ ESP / tunnel ]

udp6-multi-diffnic06
	IPv6
	IPcomp [ transport ]

udp6-multi-diffnic07
	IPv6
	IPcomp [ tunnel ]
