/*------------------------------------------------------------------------*/ /**
\defgroup doc_driver_rtc RTC Drivers


\section doc_driver_rtc_basic_and_practice RTC Basics and Best Practice

An RTC is a counter connected to a 32kHz clock source, either internal or internal.
The RTC can be used to generate periodic interrupts at a user-specified interval.

*/


