| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
FLT_EVENT_RESPONSE_s Struct Reference

`#include <fault_handler/drivers/drv_fault_handler.h>`

Collaboration diagram for FLT_EVENT_RESPONSE_s:

## Data Fields
volatile uint16_t | compareThreshold
| Signal level at which the fault condition will be detected. More...
volatile uint16_t | eventThreshold
| Bit mask will be &-ed with source as value (use 0xFFFF for full value comparison) More...
volatile uint16_t(* | ptrResponseFunction )(void)
| pointer to a user-defined function called when a defined fault monitoring event is detected More...

## Detailed Description

Definition at line 118 of file drv_fault_handler.h.

## Field Documentation

## ◆ compareThreshold

volatile uint16_t compareThreshold

Signal level at which the fault condition will be detected.

Definition at line 120 of file drv_fault_handler.h.

## ◆ eventThreshold

volatile uint16_t eventThreshold

Bit mask will be &-ed with source as value (use 0xFFFF for full value comparison)

Definition at line 121 of file drv_fault_handler.h.

## ◆ ptrResponseFunction

volatile uint16_t(* ptrResponseFunction) (void)

pointer to a user-defined function called when a defined fault monitoring event is detected

Definition at line 122 of file drv_fault_handler.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/fault_handler/drivers/drv_fault_handler.h