| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
UART_INTERFACE_s Struct Reference

`#include <common/p33c_pral/p33c_uart.h>`

Collaboration diagram for UART_INTERFACE_s:

## Data Fields
volatile struct UART_INSTANCE_STATUS_s | status
| Status word of the UART object. More...
volatile struct UART_INTERFACE_CHANNEL_s | RxD
| UART Receive Channel Configuration. More...
volatile struct UART_INTERFACE_CHANNEL_s | TxD
| UART Receive Channel Configuration. More...
volatile uint16_t | uart
| UART instance of interface. More...

## Detailed Description

Definition at line 124 of file p33c_uart.h.

## Field Documentation

## ◆ RxD

volatile struct UART_INTERFACE_CHANNEL_s RxD

UART Receive Channel Configuration.

Definition at line 126 of file p33c_uart.h.

## ◆ status

volatile struct UART_INSTANCE_STATUS_s status

Status word of the UART object.

Definition at line 125 of file p33c_uart.h.

## ◆ TxD

volatile struct UART_INTERFACE_CHANNEL_s TxD

UART Receive Channel Configuration.

Definition at line 127 of file p33c_uart.h.

## ◆ uart

volatile uint16_t uart

UART instance of interface.

Definition at line 128 of file p33c_uart.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/common/p33c_pral/p33c_uart.h