| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Low-Priority Task Execution
Firmware Architecture » Main Loop

Low priority task execution The execution of the sequence of low priority tasks is called from the main loop at lowest firmware priority #0. Tasks executed on this level may be interrupted by executions of high priority task sequences triggered by the operating system timer interrupt as well as the real-time control sytem interrupts. More...

Collaboration diagram for Low-Priority Task Execution:

Low priority task execution The execution of the sequence of low priority tasks is called from the main loop at lowest firmware priority #0. Tasks executed on this level may be interrupted by executions of high priority task sequences triggered by the operating system timer interrupt as well as the real-time control sytem interrupts.