| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
NPNZ_PORT_s Struct Reference

`#include <power_control/drivers/npnz16b.h>`

Collaboration diagram for NPNZ_PORT_s:

## Data Fields
volatile uint16_t * | ptrAddress
| Pointer to register or variable where the value is read from (e.g. ADCBUFx) or written to (e.g. PGxDC) More...
volatile int16_t | NormScaler
| Bit-shift scaler of the Q15 normalization factor. More...
volatile fractional | NormFactor
| Q15 normalization factor. More...
volatile int16_t | Offset
| Value/signal offset of this port. More...

## Detailed Description

Definition at line 226 of file npnz16b.h.

## Field Documentation

## ◆ NormFactor

volatile fractional NormFactor

Q15 normalization factor.

Definition at line 230 of file npnz16b.h.

## ◆ NormScaler

volatile int16_t NormScaler

Bit-shift scaler of the Q15 normalization factor.

Definition at line 229 of file npnz16b.h.

## ◆ Offset

volatile int16_t Offset

Value/signal offset of this port.

Definition at line 231 of file npnz16b.h.

## ◆ ptrAddress

volatile uint16_t* ptrAddress

Pointer to register or variable where the value is read from (e.g. ADCBUFx) or written to (e.g. PGxDC)

Definition at line 228 of file npnz16b.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/power_control/drivers/npnz16b.h