| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
APPTASK_STATUS_s Struct Reference

DESCRIPTION. More...

`#include <os/apptask_typedef.h>`

Collaboration diagram for APPTASK_STATUS_s:

## Data Fields
volatile bool | retval: 1
| Bit 0: Status bit indicating a failed execution of the user task. More...
volatile | unsigned: 1
| Bit 1: (reserved) More...
volatile bool | busy: 1
| Bit 7: Status bit indicating the task is busy. More...
volatile bool | enabled: 1
| Bit 15: Control bit enabling the execution of the task execute function. More...

## Detailed Description

DESCRIPTION.

Definition at line 63 of file apptask_typedef.h.

## Field Documentation

## ◆ busy

volatile bool busy

Bit 7: Status bit indicating the task is busy.

Definition at line 72 of file apptask_typedef.h.

## ◆ enabled

volatile bool enabled

Bit 15: Control bit enabling the execution of the task execute function.

Definition at line 81 of file apptask_typedef.h.

## ◆ retval

volatile bool retval

Bit 0: Status bit indicating a failed execution of the user task.

Definition at line 65 of file apptask_typedef.h.

## ◆ unsigned

volatile unsigned

Bit 1: (reserved)

Bit 14: (reserved)

Bit 13: (reserved)

Bit 12: (reserved)

Bit 11: (reserved)

Bit 10: (reserved)

Bit 9: (reserved)

Bit 8: (reserved)

Bit 6: (reserved)

Bit 5: (reserved)

Bit 4: (reserved)

Bit 3: (reserved)

Bit 2: (reserved)

Definition at line 66 of file apptask_typedef.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/os/apptask_typedef.h