| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Boost Converter
Hardware Abstraction Layer » Input Voltage Feedback » Microcontroller Abstraction

Device analog input pin, register and interrupt vector assignments of input voltage feedback signal(s) of the boost converter. More...

Collaboration diagram for Boost Converter:

#define | _BOOST_VIN_ADCInterrupt _ADCAN12Interrupt
| ADC input assignments of input voltage feedback signals. More...
#define | _BOOST_VIN_ADCISR_IF _ADCAN12IF
| ADC interrupt flag bit of the input voltage feedback channel. More...
#define | BOOST_VIN_ANSEL _ANSELC0
| GPIO analog function mode enable bit. More...
#define | BOOST_VIN_ADCCORE 8
| 0=Dedicated Core #0, 1=Dedicated Core #1, 8=Shared ADC Core More...
#define | BOOST_VIN_ADCIN 12
| Analog input number (e.g. '5' for 'AN5') More...
#define | BOOST_VIN_ADCBUF ADCBUF12
| ADC input buffer of this ADC channel. More...
#define | BOOST_VIN_ADCTRIG PG2TRIGB
| Register used for trigger placement. More...
#define | BOOST_VIN_TRGSRC BOOST_PWM_TRGSRC_TRG2
| PWM2 (=PG2) Trigger 2 via PGxTRIGB. More...

## Detailed Description

Device analog input pin, register and interrupt vector assignments of input voltage feedback signal(s) of the boost converter.

## Macro Definition Documentation

## ◆ _BOOST_VIN_ADCInterrupt

#define _BOOST_VIN_ADCInterrupt _ADCAN12Interrupt

ADC input assignments of input voltage feedback signals.

In this section the ADC input channels, related ADC result buffers, trigger sources and interrupt vectors are defined. These settings allow the fast re-assignments of feedback signals in case of hardware changes.ADC interrupt service routine function call of the input voltage feedback channel

Definition at line 1036 of file dpsk3_hwdescr.h.

## ◆ _BOOST_VIN_ADCISR_IF

#define _BOOST_VIN_ADCISR_IF _ADCAN12IF

ADC interrupt flag bit of the input voltage feedback channel.

Definition at line 1037 of file dpsk3_hwdescr.h.

## ◆ BOOST_VIN_ADCBUF

#define BOOST_VIN_ADCBUF ADCBUF12

ADC input buffer of this ADC channel.

Definition at line 1042 of file dpsk3_hwdescr.h.

## ◆ BOOST_VIN_ADCCORE

#define BOOST_VIN_ADCCORE 8

0=Dedicated Core #0, 1=Dedicated Core #1, 8=Shared ADC Core

Definition at line 1040 of file dpsk3_hwdescr.h.

## ◆ BOOST_VIN_ADCIN

#define BOOST_VIN_ADCIN 12

Analog input number (e.g. '5' for 'AN5')

Definition at line 1041 of file dpsk3_hwdescr.h.

## ◆ BOOST_VIN_ADCTRIG

#define BOOST_VIN_ADCTRIG PG2TRIGB

Register used for trigger placement.

Definition at line 1043 of file dpsk3_hwdescr.h.

## ◆ BOOST_VIN_ANSEL

#define BOOST_VIN_ANSEL _ANSELC0

GPIO analog function mode enable bit.

Definition at line 1039 of file dpsk3_hwdescr.h.

## ◆ BOOST_VIN_TRGSRC

#define BOOST_VIN_TRGSRC BOOST_PWM_TRGSRC_TRG2

PWM2 (=PG2) Trigger 2 via PGxTRIGB.

Definition at line 1044 of file dpsk3_hwdescr.h.