| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
LCD_s Struct Reference

`#include <lcd/app_lcd.h>`

Collaboration diagram for LCD_s:

## Data Fields
volatile bool | enabled
volatile uint16_t | refresh
volatile uint16_t | screen
volatile uint16_t | screens

## Detailed Description

Definition at line 54 of file app_lcd.h.

## Field Documentation

## ◆ enabled

volatile bool enabled

Definition at line 55 of file app_lcd.h.

## ◆ refresh

volatile uint16_t refresh

Definition at line 56 of file app_lcd.h.

## ◆ screen

volatile uint16_t screen

Definition at line 57 of file app_lcd.h.

## ◆ screens

volatile uint16_t screens

Definition at line 58 of file app_lcd.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/lcd/app_lcd.h