| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Structures
Here are the data structures with brief descriptions:

C ANSELx_s |
C APPLICATION_TASK_s | DESCRIPTION
C APPTASK_EXECUTION_s | DESCRIPTION
C APPTASK_STATISTICS_s | DESCRIPTION
C APPTASK_STATUS_s | DESCRIPTION
C APPTASK_TASKLINK_s | DESCRIPTION
C BOOST_ADC_INPUT_SCALING_s | ADC input signal scaling = (ADCBUF - <offset>) * <factor> >> 2^<scaler>
C BOOST_ADC_INPUT_SETTINGS_s | ADC input channel configuration
C BOOST_CONVERTER_CONSTANTS_s |
C BOOST_CONVERTER_DATA_s |
C BOOST_CONVERTER_s | BOOST control & monitoring data structure
C BOOST_CONVERTER_SETTINGS_s |
C BOOST_CONVERTER_STARTUP_s |
C BOOST_CONVERTER_STATUS_s |
C BOOST_FEEDBACK_SETTINGS_s | Boost converter feedback declarations
C BOOST_GPIO_INSTANCE_s | GPIO instance of the converter control GPIO
C BOOST_GPIO_SETTINGS_s | GPIO instance of the converter control GPIO
C BOOST_LOOP_SETTINGS_s | Boost converter main settings User defined settings for control loops;
C BOOST_STARTUP_PERIOD_HANDLER_s |
C BOOST_STARTUP_VCAP_PRECHARGE_s |
C BOOST_STATE_ID_s |
C BOOST_SWITCH_NODE_SETTINGS_s | Switching signal timing settings
C CLKDIV_s |
C CNEN0x_s |
C CNEN1x_s |
C CNFx_s |
C CNPDx_s |
C CNPUx_s |
C CNSTATx_s |
C CPU_INTTREG_s |
C CPU_RCON_s |
C DEBUGGING_LED_s |
C DEBUGGING_LED_STATUS_s |
C FAULT_MONITOR_s |
C FAULT_MONITOR_STATUS_s |
C FAULT_OBJECT_s | Generic fault object
C FLT_COMPARE_OBJECT_s |
C FLT_EVENT_RESPONSE_s |
C FLT_OBJECT_STATUS_s |
C GPIO_PORT_PIN_s |
C LATx_s |
C LCD_s |
C NPNZ16b_s |
C NPNZ_ADC_TRGCTRL_s |
C NPNZ_DATA_PROVIDERS_s |
C NPNZ_EXTENSION_HOOKS_s |
C NPNZ_FILTER_PARAMS_s |
C NPNZ_FLAGS_s | Consolidated list of status bit value enumerations
C NPNZ_GAIN_CONTROL_s |
C NPNZ_LIMITS_s |
C NPNZ_PORT_s |
C NPNZ_PORTS_s |
C NPNZ_STATUS_s |
C NPNZ_USER_DATA_BUFFER_s |
C ODCx_s |
C OS_TASK_MANAGER_s |
C OS_TASKMGR_CPU_LOAD_s | DESCRIPTION
C OS_TASKMGR_STATUS_s | Task manager data status
C OS_TASKMGR_TIMEBASE_s | DESCRIPTION
C OSCILLATOR_SYSTEM_FREQUENCIES_s |
C OSCTUN_s |
C P33C_CCP_INSTANCE_s |
C P33C_CRC_MODULE_s |
C P33C_DAC_INSTANCE_s |
C P33C_DAC_MODULE_s |
C P33C_DMA_INSTANCE_s |
C P33C_DMA_MODULE_s |
C P33C_DSP_CONFIG_s |
C P33C_GPIO_INSTANCE_s |
C P33C_OPA_MODULE_s |
C P33C_OSC_CONFIG_s |
C P33C_PMD_MODULE_s |
C P33C_PWM_GENERATOR_s |
C P33C_PWM_MODULE_s |
C P33C_TIMER_MODULE_s |
C P33C_UART_INSTANCE_s |
C PORTx_s |
C PUSH_BUTTON_OBJECT_s |
C PUSH_BUTTON_STATUS_s |
C TASK_INFO_s |
C TRAP_FLAGS_s |
C TRAP_LOGGER_s |
C TRAPLOG_STATUS_s |
C TRISx_s |
C UART_DATA_BUFFER_PROPERTY_s |
C UART_DATA_BUFFER_s |
C UART_DATBUF_STATUS_s |
C UART_INSTANCE_STATUS_s |
C UART_INTERFACE_CHANNEL_s |
C UART_INTERFACE_s |
C V_LOOP_CONTROL_LOOP_COEFFICIENTS_s |
C V_LOOP_CONTROL_LOOP_HISTORIES_s |