| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - a -

- ACoefficients : V_LOOP_CONTROL_LOOP_COEFFICIENTS_s
- ACoefficientsArraySize : NPNZ_FILTER_PARAMS_s
- ad_isns : BOOST_FEEDBACK_SETTINGS_s
- ad_temp : BOOST_FEEDBACK_SETTINGS_s
- ad_vin : BOOST_FEEDBACK_SETTINGS_s
- ad_vout : BOOST_FEEDBACK_SETTINGS_s
- adc_active : BOOST_CONVERTER_STATUS_s
- adc_buffer : BOOST_ADC_INPUT_SETTINGS_s
- adc_core : BOOST_ADC_INPUT_SETTINGS_s
- adc_input : BOOST_ADC_INPUT_SETTINGS_s
- ADCTriggerAOffset : NPNZ_ADC_TRGCTRL_s
- ADCTriggerBOffset : NPNZ_ADC_TRGCTRL_s
- ADCTriggerControl : NPNZ16b_s
- ADDRERR : TRAP_FLAGS_s
- Advanced : NPNZ16b_s
- afpllo : OSCILLATOR_SYSTEM_FREQUENCIES_s
- afvco : OSCILLATOR_SYSTEM_FREQUENCIES_s
- agc_enabled : NPNZ_STATUS_s
- AgcFactor : NPNZ_GAIN_CONTROL_s
- AgcMedian : NPNZ_GAIN_CONTROL_s
- AgcScaler : NPNZ_GAIN_CONTROL_s
- AltMaxOutput : NPNZ_LIMITS_s
- AltMinOutput : NPNZ_LIMITS_s
- AltSource : NPNZ_PORTS_s
- AltTarget : NPNZ_PORTS_s
- AmpCon1H : P33C_OPA_MODULE_s
- AmpCon1L : P33C_OPA_MODULE_s
- ANSELx : P33C_GPIO_INSTANCE_s
- ANSELx0 : ANSELx_s
- ANSELx1 : ANSELx_s
- ANSELx10 : ANSELx_s
- ANSELx11 : ANSELx_s
- ANSELx12 : ANSELx_s
- ANSELx13 : ANSELx_s
- ANSELx14 : ANSELx_s
- ANSELx15 : ANSELx_s
- ANSELx2 : ANSELx_s
- ANSELx3 : ANSELx_s
- ANSELx4 : ANSELx_s
- ANSELx5 : ANSELx_s
- ANSELx6 : ANSELx_s
- ANSELx7 : ANSELx_s
- ANSELx8 : ANSELx_s
- ANSELx9 : ANSELx_s
- APLL : TRAP_FLAGS_s
- async_mode : BOOST_CONVERTER_STATUS_s
- autorun : BOOST_CONVERTER_STATUS_s
- avg_time : APPTASK_STATISTICS_s