| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
UART_INTERFACE_CHANNEL_s Struct Reference

`#include <common/p33c_pral/p33c_uart.h>`

Collaboration diagram for UART_INTERFACE_CHANNEL_s:

## Data Fields
volatile uint16_t | dma
| DMA instance of interface. More...
volatile struct GPIO_PORT_PIN_s | io
| GPIO configuration. More...

## Detailed Description

Definition at line 118 of file p33c_uart.h.

## Field Documentation

## ◆ dma

volatile uint16_t dma

DMA instance of interface.

Definition at line 119 of file p33c_uart.h.

## ◆ io

volatile struct GPIO_PORT_PIN_s io

GPIO configuration.

Definition at line 120 of file p33c_uart.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/common/p33c_pral/p33c_uart.h