| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

FAULT_MONITOR_STATUS_s Struct Reference

`#include <fault_handler/drivers/drv_fault_handler.h>`

Collaboration diagram for FAULT_MONITOR_STATUS_s:

## Detailed Description

Definition at line 143 of file drv_fault_handler.h.

## Field Documentation

## ◆ FaultLatch

volatile bool FaultLatch

Bit 1: Flag bit indicating if a latched FAULT condition has been enforced.

Definition at line 147 of file drv_fault_handler.h.

## ◆ FaultStatus

volatile bool FaultStatus

Bit 0: Flag bit indicating if a FAULT condition has been tripped.

Definition at line 146 of file drv_fault_handler.h.

## ◆ unsigned

volatile unsigned

Bit <15:2>: (reserved)

Definition at line 148 of file drv_fault_handler.h.

## ◆ value

volatile uint16_t value

Fault monitor status word.

Definition at line 150 of file drv_fault_handler.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/fault_handler/drivers/drv_fault_handler.h