| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
BOOST_STARTUP_PERIOD_HANDLER_s Struct Reference

`#include <power_control/devices/dev_boost_typedef.h>`

Collaboration diagram for BOOST_STARTUP_PERIOD_HANDLER_s:

## Data Fields
volatile uint16_t | counter
| Soft-Start Execution Counter (read only) More...
volatile uint16_t | period
| Soft-Start Period (POD, RAMP PERIOD, PGD, etc.) More...
volatile uint16_t | reference
| Internal dummy reference used to increment/decrement controller reference. More...
volatile uint16_t | ref_inc_step
| Size/value of one reference increment/decrement or this period. More...

## Detailed Description

Definition at line 264 of file dev_boost_typedef.h.

## Field Documentation

## ◆ counter

volatile uint16_t counter

Soft-Start Execution Counter (read only)

Definition at line 266 of file dev_boost_typedef.h.

## ◆ period

volatile uint16_t period

Soft-Start Period (POD, RAMP PERIOD, PGD, etc.)

Definition at line 267 of file dev_boost_typedef.h.

## ◆ ref_inc_step

volatile uint16_t ref_inc_step

Size/value of one reference increment/decrement or this period.

Definition at line 269 of file dev_boost_typedef.h.

## ◆ reference

volatile uint16_t reference

Internal dummy reference used to increment/decrement controller reference.

Definition at line 268 of file dev_boost_typedef.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/power_control/devices/dev_boost_typedef.h