| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
P33C_DMA_INSTANCE_s Struct Reference

`#include <common/p33c_pral/p33c_dma.h>`

Collaboration diagram for P33C_DMA_INSTANCE_s:

## Data Fields
union {
volatile struct tagDMACH0BITS bits
volatile uint16_t value
} | DMACHx
union {
volatile struct tagDMAINT0BITS bits
volatile uint16_t value
} | DMAINTx
union {
struct {
uint16_t SADDR: 16
} bits
uint16_t value
} | DMASRCx
union {
struct {
uint16_t DADDR: 16
} bits
uint16_t value
} | DMADSTx
union {
struct {
uint16_t CNT: 16
} bits
uint16_t value
} | DMACNTx

## Detailed Description

Definition at line 118 of file p33c_dma.h.

## Field Documentation

## ◆ bits [1/5]

volatile struct tagDMAINT0BITS bits

Definition at line 124 of file p33c_dma.h.

## ◆ bits [2/5]

struct { ... } bits

## ◆ bits [3/5]

struct { ... } bits

## ◆ bits [4/5]

struct { ... } bits

## ◆ bits [5/5]

volatile struct tagDMACH0BITS bits

Definition at line 120 of file p33c_dma.h.

## ◆ CNT

uint16_t CNT

Definition at line 141 of file p33c_dma.h.

## ◆ DADDR

uint16_t DADDR

Definition at line 135 of file p33c_dma.h.

## ◆ DMACHx

union { ... } DMACHx

## ◆ DMACNTx

union { ... } DMACNTx

## ◆ DMADSTx

union { ... } DMADSTx

## ◆ DMAINTx

union { ... } DMAINTx

## ◆ DMASRCx

union { ... } DMASRCx

## ◆ SADDR

uint16_t SADDR

Definition at line 129 of file p33c_dma.h.

## ◆ value [1/2]

volatile uint16_t value

Definition at line 121 of file p33c_dma.h.

## ◆ value [2/2]

uint16_t value

Definition at line 131 of file p33c_dma.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/common/p33c_pral/p33c_dma.h