| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

TRAPLOG_STATUS_s Struct Reference

`#include <fault_handler/drivers/drv_trap_handler.h>`

Collaboration diagram for TRAPLOG_STATUS_s:

## Detailed Description

Definition at line 225 of file drv_trap_handler.h.

## Field Documentation

## ◆ cpu_reset_trigger

volatile bool cpu_reset_trigger

Definition at line 231 of file drv_trap_handler.h.

## ◆ sw_reset

volatile bool sw_reset

Definition at line 241 of file drv_trap_handler.h.

## ◆ unsigned

volatile unsigned

Definition at line 232 of file drv_trap_handler.h.

## ◆ value

volatile uint16_t value

Definition at line 252 of file drv_trap_handler.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/fault_handler/drivers/drv_trap_handler.h