| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Public Functions
Application Layer » Power Control Application Layer

Public functions of the application layer of the power control task. More...

Collaboration diagram for Public Functions:

Public functions of the application layer of the power control task.

The power control application layer is the proprietary user code used to configure the generic power controller device driver defined in dev_boost_typedef.h. This application layer further provides a subset of function calls allowing external software functions to control and monitor the processes of the power control device driver, such as the system-wide fault monitor or communication drivers.