| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
P33C_DMA_MODULE_s Struct Reference

`#include <common/p33c_pral/p33c_dma.h>`

Collaboration diagram for P33C_DMA_MODULE_s:

## Data Fields
union {
volatile struct tagDMACONBITS bits
volatile uint16_t value
} | DmaCon
union {
struct {
uint16_t DBUF: 16
} bits
uint16_t value
} | DmaBuf
union {
struct {
uint16_t LADDR: 16
} bits
uint16_t value
} | DmaL
union {
struct {
uint16_t HADDR: 16
} bits
uint16_t value
} | DmaH

## Detailed Description

Definition at line 60 of file p33c_dma.h.

## Field Documentation

## ◆ bits [1/4]

struct { ... } bits

## ◆ bits [2/4]

struct { ... } bits

## ◆ bits [3/4]

struct { ... } bits

## ◆ bits [4/4]

volatile struct tagDMACONBITS bits

Definition at line 62 of file p33c_dma.h.

## ◆ DBUF

uint16_t DBUF

Definition at line 67 of file p33c_dma.h.

## ◆ DmaBuf

union { ... } DmaBuf

## ◆ DmaCon

union { ... } DmaCon

## ◆ DmaH

union { ... } DmaH

## ◆ DmaL

union { ... } DmaL

## ◆ HADDR

uint16_t HADDR

Definition at line 79 of file p33c_dma.h.

## ◆ LADDR

uint16_t LADDR

Definition at line 73 of file p33c_dma.h.

## ◆ value [1/2]

volatile uint16_t value

Definition at line 63 of file p33c_dma.h.

## ◆ value [2/2]

uint16_t value

Definition at line 69 of file p33c_dma.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/common/p33c_pral/p33c_dma.h