| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
BOOST_CONVERTER_SETTINGS_s Struct Reference

`#include <power_control/devices/dev_boost_typedef.h>`

Collaboration diagram for BOOST_CONVERTER_SETTINGS_s:

## Data Fields
enum BOOST_CONTROL_MODE_e | control_mode
| Fundamental control mode. More...
volatile uint16_t | no_of_phases
| number of converter phases More...
volatile uint16_t | v_ref
| User reference setting used to control the power converter controller. More...
volatile uint16_t | i_ref
| User reference setting used to control the power converter controller. More...
volatile uint16_t | i_ref_startup
| User setting of the initial current reference at startup (used to limit startup currents) More...

## Detailed Description

Definition at line 348 of file dev_boost_typedef.h.

## Field Documentation

## ◆ control_mode

enum BOOST_CONTROL_MODE_e control_mode

Fundamental control mode.

Definition at line 350 of file dev_boost_typedef.h.

## ◆ i_ref

volatile uint16_t i_ref

User reference setting used to control the power converter controller.

Definition at line 353 of file dev_boost_typedef.h.

## ◆ i_ref_startup

volatile uint16_t i_ref_startup

User setting of the initial current reference at startup (used to limit startup currents)

Definition at line 354 of file dev_boost_typedef.h.

## ◆ no_of_phases

volatile uint16_t no_of_phases

number of converter phases

Definition at line 351 of file dev_boost_typedef.h.

## ◆ v_ref

volatile uint16_t v_ref

User reference setting used to control the power converter controller.

Definition at line 352 of file dev_boost_typedef.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/power_control/devices/dev_boost_typedef.h