| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
NPNZ_DATA_PROVIDERS_s Struct Reference

`#include <power_control/drivers/npnz16b.h>`

Collaboration diagram for NPNZ_DATA_PROVIDERS_s:

## Data Fields
volatile uint16_t * | ptrDProvControlInput
| Pointer to external data buffer of most recent, raw control input. More...
volatile uint16_t * | ptrDProvControlInputCompensated
| Pointer to external data buffer of most recent, compensated control input. More...
volatile uint16_t * | ptrDProvControlError
| Pointer to external data buffer of most recent control error. More...
volatile uint16_t * | ptrDProvControlOutput
| Pointer to external data buffer of most recent control output. More...

## Detailed Description

Definition at line 381 of file npnz16b.h.

## Field Documentation

## ◆ ptrDProvControlError

volatile uint16_t* ptrDProvControlError

Pointer to external data buffer of most recent control error.

Definition at line 385 of file npnz16b.h.

## ◆ ptrDProvControlInput

volatile uint16_t* ptrDProvControlInput

Pointer to external data buffer of most recent, raw control input.

Definition at line 383 of file npnz16b.h.

## ◆ ptrDProvControlInputCompensated

volatile uint16_t* ptrDProvControlInputCompensated

Pointer to external data buffer of most recent, compensated control input.

Definition at line 384 of file npnz16b.h.

## ◆ ptrDProvControlOutput

volatile uint16_t* ptrDProvControlOutput

Pointer to external data buffer of most recent control output.

Definition at line 386 of file npnz16b.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/power_control/drivers/npnz16b.h