| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
UART_DATA_BUFFER_s Struct Reference

`#include <common/p33c_pral/p33c_uart.h>`

Collaboration diagram for UART_DATA_BUFFER_s:

## Data Fields
volatile struct UART_DATBUF_STATUS_s | status
volatile uint8_t * | buffer
volatile uint16_t | size
volatile uint16_t | data_size
volatile uint16_t | pointer
volatile uint16_t | package_size

## Detailed Description

Definition at line 149 of file p33c_uart.h.

## Field Documentation

## ◆ buffer

volatile uint8_t* buffer

Definition at line 151 of file p33c_uart.h.

## ◆ data_size

volatile uint16_t data_size

Definition at line 153 of file p33c_uart.h.

## ◆ package_size

volatile uint16_t package_size

Definition at line 155 of file p33c_uart.h.

## ◆ pointer

volatile uint16_t pointer

Definition at line 154 of file p33c_uart.h.

## ◆ size

volatile uint16_t size

Definition at line 152 of file p33c_uart.h.

## ◆ status

volatile struct UART_DATBUF_STATUS_s status

Definition at line 150 of file p33c_uart.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/common/p33c_pral/p33c_uart.h