| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Variables
Variables & Constants
Device Driver Library Layer » Boost Converter Library » Boost Converter Library Modules » Boost Peripheral Configuration » Properties
Collaboration diagram for Variables & Constants:

## Variables
volatile uint16_t | adcore_mask =0
| This variable is use to set the ADC core mask. More...
volatile uint16_t | adcore_diff_mask =0
| This variable is use to set the ADC core mask. More...

## Detailed Description

## Variable Documentation

## ◆ adcore_diff_mask

adcore_diff_mask =0

This variable is use to set the ADC core mask.

Definition at line 32 of file dev_boost_pconfig.c.

## ◆ adcore_mask

adcore_mask =0

This variable is use to set the ADC core mask.

Definition at line 25 of file dev_boost_pconfig.c.