| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
LATx_s Struct Reference

`#include <common/p33c_pral/p33c_gpio.h>`

Collaboration diagram for LATx_s:

## Data Fields
uint16_t | LATx0:1
uint16_t | LATx1:1
uint16_t | LATx2:1
uint16_t | LATx3:1
uint16_t | LATx4:1
uint16_t | LATx5:1
uint16_t | LATx6:1
uint16_t | LATx7:1
uint16_t | LATx8:1
uint16_t | LATx9:1
uint16_t | LATx10:1
uint16_t | LATx11:1
uint16_t | LATx12:1
uint16_t | LATx13:1
uint16_t | LATx14:1
uint16_t | LATx15:1

## Detailed Description

Definition at line 111 of file p33c_gpio.h.

## Field Documentation

## ◆ LATx0

uint16_t LATx0

Definition at line 112 of file p33c_gpio.h.

## ◆ LATx1

uint16_t LATx1

Definition at line 113 of file p33c_gpio.h.

## ◆ LATx10

uint16_t LATx10

Definition at line 122 of file p33c_gpio.h.

## ◆ LATx11

uint16_t LATx11

Definition at line 123 of file p33c_gpio.h.

## ◆ LATx12

uint16_t LATx12

Definition at line 124 of file p33c_gpio.h.

## ◆ LATx13

uint16_t LATx13

Definition at line 125 of file p33c_gpio.h.

## ◆ LATx14

uint16_t LATx14

Definition at line 126 of file p33c_gpio.h.

## ◆ LATx15

uint16_t LATx15

Definition at line 127 of file p33c_gpio.h.

## ◆ LATx2

uint16_t LATx2

Definition at line 114 of file p33c_gpio.h.

## ◆ LATx3

uint16_t LATx3

Definition at line 115 of file p33c_gpio.h.

## ◆ LATx4

uint16_t LATx4

Definition at line 116 of file p33c_gpio.h.

## ◆ LATx5

uint16_t LATx5

Definition at line 117 of file p33c_gpio.h.

## ◆ LATx6

uint16_t LATx6

Definition at line 118 of file p33c_gpio.h.

## ◆ LATx7

uint16_t LATx7

Definition at line 119 of file p33c_gpio.h.

## ◆ LATx8

uint16_t LATx8

Definition at line 120 of file p33c_gpio.h.

## ◆ LATx9

uint16_t LATx9

Definition at line 121 of file p33c_gpio.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/common/p33c_pral/p33c_gpio.h