| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

drv_lcd_interface.h
1 //======================================================================================================================
2 // Copyright(c) 2018 Microchip Technology Inc. and its subsidiaries.
3 // Subject to your compliance with these terms, you may use Microchip software and any derivatives exclusively with
4 // Microchip products. It is your responsibility to comply with third party license terms applicable to your use of
5 // third-party software (including open source software) that may accompany Microchip software.
6 // THIS SOFTWARE IS SUPPLIED BY MICROCHIP "AS IS". NO WARRANTIES, WHETHER EXPRESS, IMPLIED OR STATUTORY, APPLY TO
7 // THIS SOFTWARE, INCLUDING ANY IMPLIED WARRANTIES OF NON-INFRINGEMENT, MERCHANTABILITY, AND FITNESS FOR A PARTICULAR
8 // PURPOSE.
9 // IN NO EVENT WILL MICROCHIP BE LIABLE FOR ANY INDIRECT, SPECIAL, PUNITIVE, INCIDENTAL OR CONSEQUENTIAL LOSS, DAMAGE,
10 // COST OR EXPENSE OF ANY KIND WHATSOEVER RELATED TO THE SOFTWARE, HOWEVER CAUSED, EVEN IF MICROCHIP HAS BEEN ADVISED
11 // OF THE POSSIBILITY OR THE DAMAGES ARE FORESEEABLE. TO THE FULLEST EXTENT ALLOWED BY LAW, MICROCHIP'S TOTAL LIABILITY
12 // ON ALL CLAIMS IN ANY WAY RELATED TO THIS SOFTWARE WILL NOT EXCEED THE AMOUNT OF FEES, IF ANY, THAT YOU HAVE
13 // PAID DIRECTLY TO MICROCHIP FOR THIS SOFTWARE.
14 //======================================================================================================================
15
16 //======================================================================================================================
17 // @file drv_lcd_interface.h
18 //
19 // @brief driver for the spi-interface to access the lcd controller
20 //
21 //======================================================================================================================
22
23 #ifndef _DRV_LCD_INTERFACE_H_
24 #define _DRV_LCD_INTERFACE_H_
25
26 #include <stdint.h>
27
28 extern void drv_LcdInterface_Initialize(void);
29 extern void drv_LcdInterface_Reset(void);
30 extern void drv_LcdInterface_SendCmd(const uint8_t cmd);
31 extern void drv_LcdInterface_SendChar(const char c);
32
33
34 #endif // _DRV_LCD_INTERFACE_H_