| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Modules
Boost Peripheral Configuration
Device Driver Library Layer » Boost Converter Library » Boost Converter Library Modules
Collaboration diagram for Boost Peripheral Configuration:

## Modules
| Functions
| Functions of the second library layer.
| Properties
| Properties of the second library layer.

## Detailed Description

The boost converter device driver self-manages its chip resources required to initialize and drive the converter stage and related control loops. The device driver provides standard configurations for all peripherals which are loaded into the respective Special Function Registers of each peripheral. The generic configuraitons are sublemented by the user-settings written to the converter data structure in the application layer initialization routine.