| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
NPNZ_LIMITS_s Struct Reference

`#include <power_control/drivers/npnz16b.h>`

Collaboration diagram for NPNZ_LIMITS_s:

## Data Fields
volatile int16_t | MinOutput
| Minimum output value used for clamping (R/W) More...
volatile int16_t | MaxOutput
| Maximum output value used for clamping (R/W) More...
volatile int16_t | AltMinOutput
| Alternate minimum output value used for clamping (R/W) More...
volatile int16_t | AltMaxOutput
| Alternate maximum output value used for clamping (R/W) More...

## Detailed Description

Definition at line 327 of file npnz16b.h.

## Field Documentation

## ◆ AltMaxOutput

volatile int16_t AltMaxOutput

Alternate maximum output value used for clamping (R/W)

Definition at line 332 of file npnz16b.h.

## ◆ AltMinOutput

volatile int16_t AltMinOutput

Alternate minimum output value used for clamping (R/W)

Definition at line 331 of file npnz16b.h.

## ◆ MaxOutput

volatile int16_t MaxOutput

Maximum output value used for clamping (R/W)

Definition at line 330 of file npnz16b.h.

## ◆ MinOutput

volatile int16_t MinOutput

Minimum output value used for clamping (R/W)

Definition at line 329 of file npnz16b.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/power_control/drivers/npnz16b.h