| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
BOOST_ADC_INPUT_SCALING_s Struct Reference

ADC input signal scaling = (ADCBUF - <offset>) * <factor> >> 2^<scaler> More...

`#include <power_control/devices/dev_boost_typedef.h>`

Collaboration diagram for BOOST_ADC_INPUT_SCALING_s:

## Data Fields
volatile int16_t | factor
| Fractional scaling factor (range -1 ... 0.99969) More...
volatile int16_t | scaler
| Feedback bit-shift scaler used for number normalization. More...
volatile int16_t | offset
| Signal offset as signed integer to be subtracted from ADC input. More...

## Detailed Description

ADC input signal scaling = (ADCBUF - <offset>) * <factor> >> 2^<scaler>

Definition at line 437 of file dev_boost_typedef.h.

## Field Documentation

## ◆ factor

volatile int16_t factor

Fractional scaling factor (range -1 ... 0.99969)

Definition at line 439 of file dev_boost_typedef.h.

## ◆ offset

volatile int16_t offset

Signal offset as signed integer to be subtracted from ADC input.

Definition at line 441 of file dev_boost_typedef.h.

## ◆ scaler

volatile int16_t scaler

Feedback bit-shift scaler used for number normalization.

Definition at line 440 of file dev_boost_typedef.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/power_control/devices/dev_boost_typedef.h