| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

### - e -

- early_interrupt_enable : BOOST_ADC_INPUT_SETTINGS_s
- ECCDBE : TRAP_FLAGS_s
- enabled : APPTASK_STATUS_s , BOOST_ADC_INPUT_SETTINGS_s , BOOST_CONVERTER_STATUS_s , BOOST_GPIO_INSTANCE_s , DEBUGGING_LED_STATUS_s
- Enabled : FLT_OBJECT_STATUS_s
- enabled : LCD_s , NPNZ_STATUS_s , PUSH_BUTTON_STATUS_s
- EnableInput : BOOST_GPIO_SETTINGS_s
- ErrorHistory : V_LOOP_CONTROL_LOOP_HISTORIES_s
- ErrorHistoryArraySize : NPNZ_FILTER_PARAMS_s
- event_btn_down : PUSH_BUTTON_OBJECT_s
- event_btn_up : PUSH_BUTTON_OBJECT_s
- event_long_press : PUSH_BUTTON_OBJECT_s
- event_pressed : PUSH_BUTTON_OBJECT_s
- eventThreshold : FLT_EVENT_RESPONSE_s
- exec_time : APPTASK_STATISTICS_s
- execClass : APPTASK_EXECUTION_s
- Execute : APPTASK_TASKLINK_s
- ExtensionHooks : NPNZ16b_s
- ExtHookEndOfLoopFunctionParam : NPNZ_EXTENSION_HOOKS_s
- ExtHookExitFunctionParam : NPNZ_EXTENSION_HOOKS_s
- ExtHookPreAntiWindupFunctionParam : NPNZ_EXTENSION_HOOKS_s
- ExtHookPreTargetWriteFunctionParam : NPNZ_EXTENSION_HOOKS_s
- ExtHookSourceFunctionParam : NPNZ_EXTENSION_HOOKS_s
- ExtHookStartFunctionParam : NPNZ_EXTENSION_HOOKS_s
- extr : CPU_RCON_s