| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
P33C_DAC_MODULE_s Struct Reference

`#include <common/p33c_pral/p33c_dac.h>`

Collaboration diagram for P33C_DAC_MODULE_s:

## Data Fields
union {
volatile struct tagDACCTRL1LBITS bits
volatile uint16_t value
} | DacModuleCtrl1L
volatile | unsigned: 16
union {
volatile struct tagDACCTRL2LBITS bits
volatile uint16_t value
} | DacModuleCtrl2L
union {
volatile struct tagDACCTRL2HBITS bits
volatile uint16_t value
} | DacModuleCtrl2H

## Detailed Description

Definition at line 60 of file p33c_dac.h.

## Field Documentation

## ◆ bits [1/3]

volatile struct tagDACCTRL2LBITS bits

Definition at line 67 of file p33c_dac.h.

## ◆ bits [2/3]

volatile struct tagDACCTRL1LBITS bits

Definition at line 62 of file p33c_dac.h.

## ◆ bits [3/3]

volatile struct tagDACCTRL2HBITS bits

Definition at line 71 of file p33c_dac.h.

## ◆ DacModuleCtrl1L

union { ... } DacModuleCtrl1L

## ◆ DacModuleCtrl2H

union { ... } DacModuleCtrl2H

## ◆ DacModuleCtrl2L

union { ... } DacModuleCtrl2L

## ◆ unsigned

volatile unsigned

Definition at line 65 of file p33c_dac.h.

## ◆ value

volatile uint16_t value

Definition at line 63 of file p33c_dac.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/common/p33c_pral/p33c_dac.h