| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

High-Priority Task Execution
Firmware Architecture » Main Loop

High priority task execution. More...

Collaboration diagram for High-Priority Task Execution:

High priority task execution.

The execution of the sequence of high priority tasks is triggered by the operating system timer interrupt being called on the defined priority level (default = 2). The interrupt service routine utiilzes an alternate working register set for optimum coontext management. By default, alternate working register set #1 is reserved for high priority tasks.