| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
P33C_TIMER_MODULE_s Struct Reference

`#include <common/p33c_pral/p33c_timer.h>`

Collaboration diagram for P33C_TIMER_MODULE_s:

## Data Fields
union {
struct tagT1CONBITS bits
uint16_t value
} | TxCON
volatile | unsigned:16
union {
struct {
uint16_t CNT
} bits
uint16_t value
} | TMRx
union {
struct {
uint16_t PER
} bits
uint16_t value
} | PRx

## Detailed Description

Definition at line 38 of file p33c_timer.h.

## Field Documentation

## ◆ bits [1/3]

struct { ... } bits

## ◆ bits [2/3]

struct tagT1CONBITS bits

Definition at line 41 of file p33c_timer.h.

## ◆ bits [3/3]

struct { ... } bits

## ◆ CNT

uint16_t CNT

Definition at line 49 of file p33c_timer.h.

## ◆ PER

uint16_t PER

Definition at line 58 of file p33c_timer.h.

## ◆ PRx

union { ... } PRx

## ◆ TMRx

union { ... } TMRx

## ◆ TxCON

union { ... } TxCON

## ◆ unsigned

volatile unsigned

Definition at line 45 of file p33c_timer.h.

## ◆ value

uint16_t value

Definition at line 42 of file p33c_timer.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/common/p33c_pral/p33c_timer.h