| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
BOOST_STARTUP_VCAP_PRECHARGE_s Struct Reference

`#include <power_control/devices/dev_boost_typedef.h>`

Collaboration diagram for BOOST_STARTUP_VCAP_PRECHARGE_s:

## Data Fields
volatile uint16_t | counter
| Soft-Start VCAP Charge-Up Period Counter. More...
volatile uint16_t | period
| Soft-Start VCAP Charge-Up Period (minimum time to wait when voltage has settled) More...
volatile uint16_t | timeout_counter
| Soft-Start VCAP Charge-Up Timeout Counter. More...
volatile uint16_t | timeout
| Soft-Start VCAP Charge-Up Monitor Period Counter Timeout (state machine fault state trigger) More...
volatile uint16_t | v_drop
| Acceptable voltage drop between input and output voltage when output capacitor is charging up. More...

## Detailed Description

Definition at line 287 of file dev_boost_typedef.h.

## Field Documentation

## ◆ counter

volatile uint16_t counter

Soft-Start VCAP Charge-Up Period Counter.

Definition at line 289 of file dev_boost_typedef.h.

## ◆ period

volatile uint16_t period

Soft-Start VCAP Charge-Up Period (minimum time to wait when voltage has settled)

Definition at line 290 of file dev_boost_typedef.h.

## ◆ timeout

volatile uint16_t timeout

Soft-Start VCAP Charge-Up Monitor Period Counter Timeout (state machine fault state trigger)

Definition at line 292 of file dev_boost_typedef.h.

## ◆ timeout_counter

volatile uint16_t timeout_counter

Soft-Start VCAP Charge-Up Timeout Counter.

Definition at line 291 of file dev_boost_typedef.h.

## ◆ v_drop

volatile uint16_t v_drop

Acceptable voltage drop between input and output voltage when output capacitor is charging up.

Definition at line 293 of file dev_boost_typedef.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/power_control/devices/dev_boost_typedef.h