| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - i -

- i_loop : BOOST_CONVERTER_s
- i_out : BOOST_CONVERTER_DATA_s
- i_ramp : BOOST_CONVERTER_STARTUP_s
- i_ref : BOOST_CONVERTER_SETTINGS_s
- i_ref_startup : BOOST_CONVERTER_SETTINGS_s
- i_sns : BOOST_CONVERTER_DATA_s
- idle : CPU_RCON_s
- ILR : CPU_INTTREG_s
- Initialize : APPTASK_TASKLINK_s
- interrupt_enable : BOOST_ADC_INPUT_SETTINGS_s
- inttreg : TRAP_LOGGER_s
- invert_input : NPNZ_STATUS_s
- io : UART_INTERFACE_CHANNEL_s
- io_type : BOOST_GPIO_INSTANCE_s
- iopuwr : CPU_RCON_s
- isr_timeout : OS_TASKMGR_STATUS_s