| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Modules
Main Loop
Firmware Architecture

Main Loop. More...

Collaboration diagram for Main Loop:

## Modules
| Low-Priority Task Execution
| Low priority task execution The execution of the sequence of low priority tasks is called from the main loop at lowest firmware priority #0. Tasks executed on this level may be interrupted by executions of high priority task sequences triggered by the operating system timer interrupt as well as the real-time control sytem interrupts.
| High-Priority Task Execution
| High priority task execution.

## Detailed Description

Main Loop.