| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Here is a list of all struct and union fields with links to the structures/unions they belong to:

### - r -

- rcon_reg : TRAP_LOGGER_s
- ready : BOOST_CONVERTER_STATUS_s , UART_INSTANCE_STATUS_s
- RecoveryResponse : FAULT_OBJECT_s
- ref_inc_step : BOOST_STARTUP_PERIOD_HANDLER_s
- reference : BOOST_LOOP_SETTINGS_s , BOOST_STARTUP_PERIOD_HANDLER_s
- ReferenceObject : FAULT_OBJECT_s
- refresh : LCD_s
- reset_count : TRAP_LOGGER_s
- retval : APPTASK_STATUS_s
- ROI : CLKDIV_s
- rpid : GPIO_PORT_PIN_s
- rx_buffer : UART_DATA_BUFFER_PROPERTY_s
- rx_use_dma : UART_INSTANCE_STATUS_s
- RXCHK : P33C_UART_INSTANCE_s
- RxD : UART_INTERFACE_s
- RXREG : P33C_UART_INSTANCE_s