| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
CNEN0x_s Struct Reference

`#include <common/p33c_pral/p33c_gpio.h>`

Collaboration diagram for CNEN0x_s:

## Data Fields
uint16_t | CNEN0x0:1
uint16_t | CNEN0x1:1
uint16_t | CNEN0x2:1
uint16_t | CNEN0x3:1
uint16_t | CNEN0x4:1
uint16_t | CNEN0x5:1
uint16_t | CNEN0x6:1
uint16_t | CNEN0x7:1
uint16_t | CNEN0x8:1
uint16_t | CNEN0x9:1
uint16_t | CNEN0x10:1
uint16_t | CNEN0x11:1
uint16_t | CNEN0x12:1
uint16_t | CNEN0x13:1
uint16_t | CNEN0x14:1
uint16_t | CNEN0x15:1

## Detailed Description

Definition at line 191 of file p33c_gpio.h.

## Field Documentation

## ◆ CNEN0x0

uint16_t CNEN0x0

Definition at line 192 of file p33c_gpio.h.

## ◆ CNEN0x1

uint16_t CNEN0x1

Definition at line 193 of file p33c_gpio.h.

## ◆ CNEN0x10

uint16_t CNEN0x10

Definition at line 202 of file p33c_gpio.h.

## ◆ CNEN0x11

uint16_t CNEN0x11

Definition at line 203 of file p33c_gpio.h.

## ◆ CNEN0x12

uint16_t CNEN0x12

Definition at line 204 of file p33c_gpio.h.

## ◆ CNEN0x13

uint16_t CNEN0x13

Definition at line 205 of file p33c_gpio.h.

## ◆ CNEN0x14

uint16_t CNEN0x14

Definition at line 206 of file p33c_gpio.h.

## ◆ CNEN0x15

uint16_t CNEN0x15

Definition at line 207 of file p33c_gpio.h.

## ◆ CNEN0x2

uint16_t CNEN0x2

Definition at line 194 of file p33c_gpio.h.

## ◆ CNEN0x3

uint16_t CNEN0x3

Definition at line 195 of file p33c_gpio.h.

## ◆ CNEN0x4

uint16_t CNEN0x4

Definition at line 196 of file p33c_gpio.h.

## ◆ CNEN0x5

uint16_t CNEN0x5

Definition at line 197 of file p33c_gpio.h.

## ◆ CNEN0x6

uint16_t CNEN0x6

Definition at line 198 of file p33c_gpio.h.

## ◆ CNEN0x7

uint16_t CNEN0x7

Definition at line 199 of file p33c_gpio.h.

## ◆ CNEN0x8

uint16_t CNEN0x8

Definition at line 200 of file p33c_gpio.h.

## ◆ CNEN0x9

uint16_t CNEN0x9

Definition at line 201 of file p33c_gpio.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/common/p33c_pral/p33c_gpio.h