| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
FLT_COMPARE_OBJECT_s Struct Reference

`#include <fault_handler/drivers/drv_fault_handler.h>`

Collaboration diagram for FLT_COMPARE_OBJECT_s:

## Data Fields
volatile uint16_t * | ptrObject
| Pointer to register or variable which should be monitored. More...
volatile uint16_t | bitMask
| Bit mask will be &-ed with source as value (use 0xFFFF for full value comparison) More...

## Detailed Description

Definition at line 104 of file drv_fault_handler.h.

## Field Documentation

## ◆ bitMask

volatile uint16_t bitMask

Bit mask will be &-ed with source as value (use 0xFFFF for full value comparison)

Definition at line 107 of file drv_fault_handler.h.

## ◆ ptrObject

volatile uint16_t* ptrObject

Pointer to register or variable which should be monitored.

Definition at line 106 of file drv_fault_handler.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/fault_handler/drivers/drv_fault_handler.h