| Digital Power Starter Kit 3 Firmware dsPIC33C Boost Converter Voltage Mode Control Example |

Data Fields
BOOST_GPIO_SETTINGS_s Struct Reference

GPIO instance of the converter control GPIO. More...

`#include <power_control/devices/dev_boost_typedef.h>`

Collaboration diagram for BOOST_GPIO_SETTINGS_s:

## Data Fields
volatile struct BOOST_GPIO_INSTANCE_s | EnableInput
| External ENABLE input. More...
volatile struct BOOST_GPIO_INSTANCE_s | PowerGood
| Power Good Output. More...

## Detailed Description

GPIO instance of the converter control GPIO.

Definition at line 514 of file dev_boost_typedef.h.

## Field Documentation

## ◆ EnableInput

volatile struct BOOST_GPIO_INSTANCE_s EnableInput

External ENABLE input.

Definition at line 516 of file dev_boost_typedef.h.

## ◆ PowerGood

volatile struct BOOST_GPIO_INSTANCE_s PowerGood

Power Good Output.

Definition at line 517 of file dev_boost_typedef.h.

The documentation for this struct was generated from the following file:

- dpsk_boost_vmc.X/sources/power_control/devices/dev_boost_typedef.h